**DESCRIPTION:**

cross-band repeating is an effective way to extend the range of your handheld radio. The cross-band repeat function works by using a dual band mobile or base radio to retransmit on one frequency band a signal received on another frequency band, and vice versa. A common use of the cross band repeat is to extend your range of a handheld radio by using the higher power of your dual band mobile transceiver to hit a distant repeater.

Weight: 65gr

Voltage: 5V

Power output: 0.8-1W

RF Connectors: SMA

